Kernel: Linux francesco 2.6.8-2-386 #1 Thu May 19 17:40:50 JST 2005 i686 GNU/Linux

Questo è l'estratto del mio /var/log/messages:

(a pag. 10 c'è la lista dei moduli caricati)

Oct 30 19:33:16 localhost syslogd 1.4.1#17: restart.

Oct 30 19:33:16 localhost kernel: klogd 1.4.1#17, log source = /proc/kmsg started.

Oct 30 19:33:16 localhost kernel: Inspecting /boot/System.map-2.6.8-2-386

Oct 30 19:33:16 localhost kernel: Loaded 28182 symbols from /boot/System.map-2.6.8-2-386.

Oct 30 19:33:16 localhost kernel: Symbols match kernel version 2.6.8.

Oct 30 19:33:16 localhost kernel: No module symbols loaded - kernel modules not enabled.

Oct 30 19:33:16 localhost kernel: Linux version 2.6.8-2-386 (horms@tabatha.lab.ultramonkey.org) (gcc version 3.3.5 (Debian 1:3.3.5-12)) #1 Thu May 19 17:40:50 JST 2005

Oct 30 19:33:16 localhost kernel: BIOS-provided physical RAM map:

Oct 30 19:33:16 localhost kernel: BIOS-e820: 0000000000000000 - 000000000009fc00 (usable)

Oct 30 19:33:16 localhost kernel: BIOS-e820: 000000000009fc00 - 00000000000a0000 (reserved)

Oct 30 19:33:16 localhost kernel: BIOS-e820: 00000000000e0000 - 0000000000100000 (reserved)

Oct 30 19:33:16 localhost kernel: BIOS-e820: 0000000000100000 - 000000000dff0000 (usable)

Oct 30 19:33:16 localhost kernel: BIOS-e820: 000000000dff0000 - 000000000dffffc0 (ACPI data)

Oct 30 19:33:16 localhost kernel: BIOS-e820: 000000000dffffc0 - 000000000e000000 (ACPI NVS)

Oct 30 19:33:16 localhost kernel: BIOS-e820: 00000000fff80000 - 0000000100000000 (reserved)

Oct 30 19:33:16 localhost kernel: 223MB LOWMEM available.

Oct 30 19:33:16 localhost kernel: DMI 2.3 present.

Oct 30 19:33:16 localhost kernel: ACPI: RSDP (v000 OID_00 ) @ 0x000e5010

Oct 30 19:33:16 localhost kernel: ACPI: RSDT (v001 INSYDE RSDT_000 0x00000001 _CSI 0x00010100) @ 0x0dfffbc0

Oct 30 19:33:16 localhost kernel: ACPI: FADT (v001 INSYDE FACP_000 0x00000100 _CSI 0x00010100) @ 0x0dfffac0

Oct 30 19:33:16 localhost kernel: ACPI: BOOT (v001 INSYDE SYS_BOOT 0x00000100 _CSI 0x00010100) @ 0x0dfffb50

Oct 30 19:33:16 localhost kernel: ACPI: DBGP (v001 INSYDE DBGP_000 0x00000100 _CSI 0x00010100) @ 0x0dfffb80

Oct 30 19:33:16 localhost kernel: ACPI: DSDT (v001 INSYDE VT8372 0x00001000 INTL 0x02002025) @ 0x00000000

Oct 30 19:33:16 localhost kernel: ACPI: PM-Timer IO Port: 0x1008

Oct 30 19:33:16 localhost kernel: Built 1 zonelists

Oct 30 19:33:16 localhost kernel: Kernel command line: root=/dev/hda2 ro

Oct 30 19:33:16 localhost kernel: Local APIC disabled by BIOS -- reenabling.

Oct 30 19:33:16 localhost kernel: Found and enabled local APIC!

Oct 30 19:33:16 localhost kernel: Initializing CPU#0

Oct 30 19:33:16 localhost kernel: PID hash table entries: 1024 (order 10: 8192 bytes)

Oct 30 19:33:16 localhost kernel: Detected 1658.233 MHz processor.

Oct 30 19:33:16 localhost kernel: Using pmtmr for high-res timesource

Oct 30 19:33:16 localhost kernel: Console: colour VGA+ 80x25

Oct 30 19:33:16 localhost kernel: Dentry cache hash table entries: 32768 (order: 5, 131072 bytes)

Oct 30 19:33:16 localhost kernel: Inode-cache hash table entries: 16384 (order: 4, 65536 bytes)

Oct 30 19:33:16 localhost kernel: Memory: 219900k/229312k available (1336k kernel code, 8724k reserved, 732k data, 204k init, 0k highmem)

Oct 30 19:33:16 localhost kernel: Checking if this processor honours the WP bit even in supervisor mode... Ok.

Oct 30 19:33:16 localhost kernel: Calibrating delay loop... 3244.03 BogoMIPS

Oct 30 19:33:16 localhost kernel: Security Scaffold v1.0.0 initialized

Oct 30 19:33:16 localhost kernel: Mount-cache hash table entries: 512 (order: 0, 4096 bytes)

Oct 30 19:33:16 localhost kernel: CPU: L1 I Cache: 64K (64 bytes/line), D cache 64K (64 bytes/line)

Oct 30 19:33:16 localhost kernel: CPU: L2 Cache: 256K (64 bytes/line)

Oct 30 19:33:16 localhost kernel: CPU: AMD mobile AMD Athlon(tm) XP-M 2000+ stepping 01

Oct 30 19:33:16 localhost kernel: Enabling fast FPU save and restore... done.

Oct 30 19:33:16 localhost kernel: Enabling unmasked SIMD FPU exception support... done.

Oct 30 19:33:16 localhost kernel: Checking 'hlt' instruction... OK.

Oct 30 19:33:16 localhost kernel: Checking for popad bug... OK.

Oct 30 19:33:16 localhost kernel: enabled ExtINT on CPU#0

Oct 30 19:33:16 localhost kernel: ESR value before enabling vector: 00000000

Oct 30 19:33:16 localhost kernel: ESR value after enabling vector: 00000000

Oct 30 19:33:16 localhost kernel: Using local APIC timer interrupts.

Oct 30 19:33:16 localhost kernel: calibrating APIC timer ...

Oct 30 19:33:16 localhost kernel: ..... CPU clock speed is 1657.0884 MHz.

Oct 30 19:33:16 localhost kernel: ..... host bus clock speed is 264.0200 MHz.

Oct 30 19:33:16 localhost kernel: checking if image is initramfs...it isn't (ungzip failed); looks like an initrd

Oct 30 19:33:16 localhost kernel: Freeing initrd memory: 4216k freed

Oct 30 19:33:16 localhost kernel: NET: Registered protocol family 16

Oct 30 19:33:16 localhost kernel: EISA bus registered

Oct 30 19:33:16 localhost kernel: PCI: PCI BIOS revision 2.10 entry at 0xe8b24, last bus=1

Oct 30 19:33:16 localhost kernel: PCI: Using configuration type 1

Oct 30 19:33:16 localhost kernel: mtrr: v2.0 (20020519)

Oct 30 19:33:16 localhost kernel: ACPI: Subsystem revision 20040326

Oct 30 19:33:16 localhost kernel: ACPI: IRQ9 SCI: Edge set to Level Trigger.

Oct 30 19:33:16 localhost kernel: spurious 8259A interrupt: IRQ7.

Oct 30 19:33:16 localhost kernel: ACPI: Interpreter enabled

Oct 30 19:33:16 localhost kernel: ACPI: Using PIC for interrupt routing

Oct 30 19:33:16 localhost kernel: ACPI: PCI Root Bridge [PCI0] (00:00)

Oct 30 19:33:16 localhost kernel: PCI: Probing PCI hardware (bus 00)

Oct 30 19:33:16 localhost kernel: ACPI: Embedded Controller [EC0] (gpe 5)

Oct 30 19:33:16 localhost kernel: ACPI: PCI Interrupt Link [LNKA] (IRQs 5 7 *10 11)

Oct 30 19:33:16 localhost kernel: ACPI: PCI Interrupt Link [LNKB] (IRQs 7) *11

Oct 30 19:33:16 localhost kernel: ACPI: PCI Interrupt Link [LNKC] (IRQs *5 7 10 11)

Oct 30 19:33:16 localhost kernel: ACPI: PCI Interrupt Link [LNKD] (IRQs 5 7 10 *11)

Oct 30 19:33:16 localhost kernel: Linux Plug and Play Support v0.97 (c) Adam Belay

Oct 30 19:33:16 localhost kernel: PnPBIOS: Scanning system for PnP BIOS support...

Oct 30 19:33:16 localhost kernel: PnPBIOS: Found PnP BIOS installation structure at 0xc00ff020

Oct 30 19:33:16 localhost kernel: PnPBIOS: PnP BIOS version 1.0, entry 0xea000:0x372a, dseg 0xea000

Oct 30 19:33:16 localhost kernel: PCI: Using ACPI for IRQ routing

Oct 30 19:33:16 localhost kernel: ACPI: PCI Interrupt Link [LNKB] enabled at IRQ 7

Oct 30 19:33:16 localhost kernel: ACPI: PCI interrupt 0000:00:09.0[A] -> GSI 7 (level, low) -> IRQ 7

Oct 30 19:33:16 localhost kernel: ACPI: PCI interrupt 0000:00:09.1[B] -> GSI 7 (level, low) -> IRQ 7

Oct 30 19:33:16 localhost kernel: ACPI: PCI Interrupt Link [LNKC] enabled at IRQ 5

Oct 30 19:33:16 localhost kernel: ACPI: PCI interrupt 0000:00:0b.0[A] -> GSI 5 (level, low) -> IRQ 5

Oct 30 19:33:16 localhost kernel: ACPI: PCI Interrupt Link [LNKA] enabled at IRQ 10

Oct 30 19:33:16 localhost kernel: ACPI: PCI interrupt 0000:00:10.0[A] -> GSI 10 (level, low) -> IRQ 10

Oct 30 19:33:16 localhost kernel: ACPI: PCI interrupt 0000:00:10.1[B] -> GSI 7 (level, low) -> IRQ 7

Oct 30 19:33:16 localhost kernel: ACPI: PCI Interrupt Link [LNKD] enabled at IRQ 11

Oct 30 19:33:16 localhost kernel: ACPI: PCI interrupt 0000:00:10.3[D] -> GSI 11 (level, low) -> IRQ 11

Oct 30 19:33:16 localhost kernel: ACPI: PCI interrupt 0000:00:11.1[A]: no GSI

Oct 30 19:33:16 localhost kernel: ACPI: PCI interrupt 0000:00:11.5[C] -> GSI 5 (level, low) -> IRQ 5

Oct 30 19:33:16 localhost kernel: ACPI: PCI interrupt 0000:00:11.6[C] -> GSI 5 (level, low) -> IRQ 5

Oct 30 19:33:16 localhost kernel: ACPI: PCI interrupt 0000:00:12.0[A] -> GSI 10 (level, low) -> IRQ 10

Oct 30 19:33:16 localhost kernel: ACPI: PCI interrupt 0000:01:00.0[A] -> GSI 10 (level, low) -> IRQ 10

Oct 30 19:33:16 localhost kernel: Simple Boot Flag at 0x37 set to 0x1

Oct 30 19:33:16 localhost kernel: VFS: Disk quotas dquot_6.5.1

Oct 30 19:33:16 localhost kernel: Dquot-cache hash table entries: 1024 (order 0, 4096 bytes)

Oct 30 19:33:16 localhost kernel: devfs: 2004-01-31 Richard Gooch (rgooch@atnf.csiro.au)

Oct 30 19:33:16 localhost kernel: devfs: boot_options: 0x0

Oct 30 19:33:16 localhost kernel: Initializing Cryptographic API

Oct 30 19:33:16 localhost kernel: PCI: Via IRQ fixup for 0000:00:10.1, from 11 to 7

Oct 30 19:33:16 localhost kernel: isapnp: Scanning for PnP cards...

Oct 30 19:33:16 localhost kernel: isapnp: No Plug & Play device found

Oct 30 19:33:16 localhost kernel: Serial: 8250/16550 driver $Revision: 1.90 $ 54 ports, IRQ sharing enabled

Oct 30 19:33:16 localhost kernel: RAMDISK driver initialized: 16 RAM disks of 8192K size 1024 blocksize

Oct 30 19:33:16 localhost kernel: serio: i8042 AUX port at 0x60,0x64 irq 12

Oct 30 19:33:16 localhost kernel: serio: i8042 KBD port at 0x60,0x64 irq 1

Oct 30 19:33:16 localhost kernel: input: AT Translated Set 2 keyboard on isa0060/serio0

Oct 30 19:33:16 localhost kernel: EISA: Probing bus 0 at eisa0

Oct 30 19:33:16 localhost kernel: EISA: Detected 0 cards.

Oct 30 19:33:16 localhost kernel: NET: Registered protocol family 2

Oct 30 19:33:16 localhost kernel: IP: routing cache hash table of 2048 buckets, 16Kbytes

Oct 30 19:33:16 localhost kernel: TCP: Hash tables configured (established 16384 bind 32768)

Oct 30 19:33:16 localhost kernel: NET: Registered protocol family 8

Oct 30 19:33:16 localhost kernel: NET: Registered protocol family 20

Oct 30 19:33:16 localhost kernel: ACPI: (supports S0 S3 S4 S5)

Oct 30 19:33:16 localhost kernel: RAMDISK: cramfs filesystem found at block 0

Oct 30 19:33:16 localhost kernel: RAMDISK: Loading 4216 blocks [1 disk] into ram disk... |^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^H|^H/^H-^H\^Hdone.

Oct 30 19:33:16 localhost kernel: VFS: Mounted root (cramfs filesystem) readonly.

Oct 30 19:33:16 localhost kernel: Freeing unused kernel memory: 204k freed

Oct 30 19:33:16 localhost kernel: vesafb: probe of vesafb0 failed with error -6

Oct 30 19:33:16 localhost kernel: NET: Registered protocol family 1

Oct 30 19:33:16 localhost kernel: Uniform Multi-Platform E-IDE driver Revision: 7.00alpha2

Oct 30 19:33:16 localhost kernel: ide: Assuming 33MHz system bus speed for PIO modes; override with idebus=xx

Oct 30 19:33:16 localhost kernel: VP_IDE: IDE controller at PCI slot 0000:00:11.1

Oct 30 19:33:16 localhost kernel: ACPI: PCI interrupt 0000:00:11.1[A]: no GSI

Oct 30 19:33:16 localhost kernel: VP_IDE: chipset revision 6

Oct 30 19:33:16 localhost kernel: VP_IDE: not 100%% native mode: will probe irqs later

Oct 30 19:33:16 localhost kernel: VP_IDE: VIA vt8235 (rev 00) IDE UDMA133 controller on pci0000:00:11.1

Oct 30 19:33:16 localhost kernel: ide0: BM-DMA at 0x1100-0x1107, BIOS settings: hda:DMA, hdb:pio

Oct 30 19:33:16 localhost kernel: ide1: BM-DMA at 0x1108-0x110f, BIOS settings: hdc:DMA, hdd:pio

Oct 30 19:33:16 localhost kernel: hda: FUJITSU MHT2030AT, ATA DISK drive

Oct 30 19:33:16 localhost kernel: Using anticipatory io scheduler

Oct 30 19:33:16 localhost kernel: ide0 at 0x1f0-0x1f7,0x3f6 on irq 14

Oct 30 19:33:16 localhost kernel: hda: max request size: 128KiB

Oct 30 19:33:16 localhost kernel: hda: 58605120 sectors (30005 MB) w/2048KiB Cache, CHS=58140/16/63, UDMA(100)

Oct 30 19:33:16 localhost kernel: /dev/ide/host0/bus0/target0/lun0: p1 p2 p3 < p5 >

Oct 30 19:33:16 localhost kernel: hdc: TOSHIBA DVD-ROM SD-R6012, ATAPI CD/DVD-ROM drive

Oct 30 19:33:16 localhost kernel: ide1 at 0x170-0x177,0x376 on irq 15

Oct 30 19:33:16 localhost kernel: kjournald starting. Commit interval 5 seconds

Oct 30 19:33:16 localhost kernel: EXT3-fs: mounted filesystem with ordered data mode.

Oct 30 19:33:16 localhost kernel: Adding 618460k swap on /dev/hda5. Priority:-1 extents:1

Oct 30 19:33:16 localhost kernel: EXT3 FS on hda2, internal journal

Oct 30 19:33:16 localhost kernel: hdc: ATAPI 24X DVD-ROM DVD-R CD-R/RW drive, 2048kB Cache, UDMA(33)

Oct 30 19:33:16 localhost kernel: Uniform CD-ROM driver Revision: 3.20

Oct 30 19:33:16 localhost kernel: Synaptics Touchpad, model: 1

Oct 30 19:33:16 localhost kernel: Firmware: 5.9

Oct 30 19:33:16 localhost kernel: Sensor: 37

Oct 30 19:33:16 localhost kernel: new absolute packet format

Oct 30 19:33:16 localhost kernel: Touchpad has extended capability bits

Oct 30 19:33:16 localhost kernel: -> multifinger detection

Oct 30 19:33:16 localhost kernel: -> palm detection

Oct 30 19:33:16 localhost kernel: input: SynPS/2 Synaptics TouchPad on isa0060/serio1

Oct 30 19:33:16 localhost kernel: SCSI subsystem initialized

Oct 30 19:33:16 localhost kernel: sbp2: $Rev: 1219 $ Ben Collins <bcollins@debian.org>

Oct 30 19:33:16 localhost kernel: CSLIP: code copyright 1989 Regents of the University of California

Oct 30 19:33:16 localhost kernel: PPP generic driver version 2.4.2

Oct 30 19:33:16 localhost kernel: usbcore: registered new driver usbfs

Oct 30 19:33:16 localhost kernel: usbcore: registered new driver hub

Oct 30 19:33:16 localhost kernel: mice: PS/2 mouse device common for all mice

Oct 30 19:33:16 localhost kernel: Capability LSM initialized

Oct 30 19:33:16 localhost kernel: ts: Compaq touchscreen protocol output

Oct 30 19:33:16 localhost kernel: ohci1394: $Rev: 1223 $ Ben Collins <bcollins@debian.org>

Oct 30 19:33:16 localhost kernel: ACPI: PCI interrupt 0000:00:0b.0[A] -> GSI 5 (level, low) -> IRQ 5

Oct 30 19:33:16 localhost kernel: ohci1394: fw-host0: OHCI-1394 1.0 (PCI): IRQ=[5] MMIO=[fedff800-fedfffff] Max Packet=[2048]

Oct 30 19:33:16 localhost kernel: NET: Registered protocol family 23

Oct 30 19:33:16 localhost kernel: via-rhine.c:v1.10-LK1.1.20-2.6 May-23-2004 Written by Donald Becker

Oct 30 19:33:16 localhost kernel: ACPI: PCI interrupt 0000:00:12.0[A] -> GSI 10 (level, low) -> IRQ 10

Oct 30 19:33:16 localhost kernel: eth0: VIA Rhine II at 0xe300, 00:40:d0:3c:ed:52, IRQ 10.

Oct 30 19:33:16 localhost kernel: eth0: MII PHY found at address 1, status 0x7849 advertising 05e1 Link 0000.

Oct 30 19:33:16 localhost kernel: Via 686a/8233/8235 audio driver 1.9.1-ac4-2.5

Oct 30 19:33:16 localhost kernel: ACPI: PCI interrupt 0000:00:11.5[C] -> GSI 5 (level, low) -> IRQ 5

Oct 30 19:33:16 localhost kernel: via82cxxx: Six channel audio available

Oct 30 19:33:16 localhost kernel: ac97_codec: AC97 Audio codec, id: ALG16 (ALC200/200P)

Oct 30 19:33:16 localhost kernel: via82cxxx: board #1 at 0xE100, IRQ 5

Oct 30 19:33:16 localhost kernel: USB Universal Host Controller Interface driver v2.2

Oct 30 19:33:16 localhost kernel: ACPI: PCI interrupt 0000:00:10.0[A] -> GSI 10 (level, low) -> IRQ 10

Oct 30 19:33:16 localhost kernel: uhci_hcd 0000:00:10.0: VIA Technologies, Inc. VT82xxxxx UHCI USB 1.1 Controller

Oct 30 19:33:16 localhost kernel: uhci_hcd 0000:00:10.0: irq 10, io base 00001200

Oct 30 19:33:16 localhost kernel: uhci_hcd 0000:00:10.0: new USB bus registered, assigned bus number 1

Oct 30 19:33:16 localhost kernel: hub 1-0:1.0: USB hub found

Oct 30 19:33:16 localhost kernel: hub 1-0:1.0: 2 ports detected

Oct 30 19:33:16 localhost kernel: ACPI: PCI interrupt 0000:00:10.1[B] -> GSI 7 (level, low) -> IRQ 7

Oct 30 19:33:16 localhost kernel: uhci_hcd 0000:00:10.1: VIA Technologies, Inc. VT82xxxxx UHCI USB 1.1 Controller (#2)

Oct 30 19:33:16 localhost kernel: uhci_hcd 0000:00:10.1: irq 7, io base 00001300

Oct 30 19:33:16 localhost kernel: uhci_hcd 0000:00:10.1: new USB bus registered, assigned bus number 2

Oct 30 19:33:16 localhost kernel: hub 2-0:1.0: USB hub found

Oct 30 19:33:16 localhost kernel: ip1394: $Rev: 1224 $ Ben Collins <bcollins@debian.org>

Oct 30 19:33:16 localhost kernel: hub 2-0:1.0: 2 ports detected

Oct 30 19:33:16 localhost kernel: ACPI: PCI interrupt 0000:00:10.3[D] -> GSI 11 (level, low) -> IRQ 11

Oct 30 19:33:16 localhost kernel: ehci_hcd 0000:00:10.3: VIA Technologies, Inc. USB 2.0

Oct 30 19:33:16 localhost kernel: ehci_hcd 0000:00:10.3: irq 11, pci mem cea4f000

Oct 30 19:33:16 localhost kernel: ehci_hcd 0000:00:10.3: new USB bus registered, assigned bus number 3

Oct 30 19:33:16 localhost kernel: ehci_hcd 0000:00:10.3: USB 2.0 enabled, EHCI 1.00, driver 2004-May-10

Oct 30 19:33:16 localhost kernel: hub 3-0:1.0: USB hub found

Oct 30 19:33:16 localhost kernel: hub 3-0:1.0: 4 ports detected

Oct 30 19:33:16 localhost kernel: Linux agpgart interface v0.100 (c) Dave Jones

Oct 30 19:33:16 localhost kernel: agpgart: Detected VIA Apollo Pro266 chipset

Oct 30 19:33:16 localhost kernel: agpgart: Maximum main memory to use for agp memory: 176M

Oct 30 19:33:16 localhost kernel: agpgart: AGP aperture is 64M @ 0xa0000000

Oct 30 19:33:16 localhost kernel: cpci_hotplug: CompactPCI Hot Plug Core version: 0.2

Oct 30 19:33:16 localhost kernel: pci_hotplug: PCI Hot Plug PCI Core version: 0.5

Oct 30 19:33:16 localhost kernel: Linux Kernel Card Services

Oct 30 19:33:16 localhost kernel: options: [pci] [cardbus] [pm]

Oct 30 19:33:16 localhost kernel: ACPI: PCI interrupt 0000:00:09.0[A] -> GSI 7 (level, low) -> IRQ 7

Oct 30 19:33:16 localhost kernel: Yenta: CardBus bridge found at 0000:00:09.0 [1631:e004]

Oct 30 19:33:16 localhost kernel: Yenta: ISA IRQ mask 0x0040, PCI irq 7

Oct 30 19:33:16 localhost kernel: Socket status: 30000006

Oct 30 19:33:16 localhost kernel: NET: Registered protocol family 17

Oct 30 19:33:17 localhost kernel: ACPI: Battery Slot [BAT0] (battery present)

Oct 30 19:33:17 localhost kernel: ACPI: AC Adapter [AC] (off-line)

Oct 30 19:33:17 localhost kernel: ACPI: Processor [CPU0] (supports C1 C2)

Oct 30 19:33:17 localhost kernel: ACPI: Power Button (FF) [PWRF]

Oct 30 19:33:17 localhost kernel: ACPI: Sleep Button (CM) [SBTN]

Oct 30 19:33:17 localhost kernel: ACPI: Lid Switch [LID]

Oct 30 19:33:20 localhost kernel: lp: driver loaded but no devices found

Oct 30 19:33:22 localhost kernel: NET: Registered protocol family 10

Oct 30 19:33:22 localhost kernel: Disabled Privacy Extensions on device c02cc960(lo)

Oct 30 19:33:22 localhost kernel: IPv6 over IPv4 tunneling driver

Oct 30 19:33:23 localhost kernel: cs: IO port probe 0x0100-0x04ff: excluding 0x4d0-0x4d7

Oct 30 19:33:23 localhost kernel: cs: IO port probe 0x0800-0x08ff: clean.

Oct 30 19:33:23 localhost kernel: cs: IO port probe 0x0c00-0x0cff: clean.

Oct 30 19:33:23 localhost kernel: cs: IO port probe 0x0a00-0x0aff: clean.

Oct 30 19:33:29 localhost kernel: mtrr: no more MTRRs available

Oct 30 19:33:29 localhost last message repeated 3 times

Oct 30 19:33:41 localhost gconfd (francesco-3380): Inizializzazione (versione 2.8.1), pid 3380, utente 'francesco'

Oct 30 19:33:41 localhost gconfd (francesco-3380): L'indirizzo "xml:readonly:/etc/gconf/gconf.xml.mandatory" è stato risolta ad una fonte di configurazione in sola lettura in posizione 0

Oct 30 19:33:41 localhost gconfd (francesco-3380): L'indirizzo "xml:readwrite:/home/francesco/.gconf" è stato risolto ad una fonte di configurazione scrivibile in posizione 1

Oct 30 19:33:41 localhost gconfd (francesco-3380): L'indirizzo "xml:readonly:/etc/gconf/gconf.xml.defaults" è stato risolta ad una fonte di configurazione in sola lettura in posizione 2

Oct 30 19:33:58 localhost gconfd (francesco-3380): L'indirizzo "xml:readwrite:/home/francesco/.gconf" è stato risolto ad una fonte di configurazione scrivibile in posizione 0

Oct 30 19:35:45 localhost kernel: usb 2-2: new full speed USB device using address 2

Oct 30 19:35:46 localhost kernel: usb 2-2: new full speed USB device using address 3

Oct 30 19:35:48 localhost usb.agent[3568]: speedtch: loaded successfully

Oct 30 19:35:48 localhost kernel: usbcore: registered new driver speedtch

Oct 30 19:35:48 localhost usb.agent[3562]: speedtch: already loaded

Oct 30 19:35:48 localhost usb.agent[3576]: speedtch: already loaded

Oct 30 19:35:48 localhost usb.agent[3562]: speedtouch: loaded successfully

Oct 30 19:35:49 localhost usb.agent[3568]: speedtouch: loaded successfully

Oct 30 19:35:49 localhost usb.agent[3576]: speedtouch: loaded successfully

Oct 30 19:35:49 localhost modem_run[3773]: modem_run version 1.3.1 started by root uid 0

Oct 30 19:35:49 localhost modem_run[3775]: modem_run version 1.3.1 started by root uid 0

Oct 30 19:35:49 localhost modem_run[3779]: modem_run version 1.3.1 started by root uid 0

Oct 30 19:35:51 localhost kernel: usb 2-2: bulk timeout on ep5in

Oct 30 19:35:51 localhost kernel: usb 2-2: usbfs: USBDEVFS_BULK failed ep 0x85 len 512 ret -110

Oct 30 19:36:07 localhost gconfd (root-3801): Inizializzazione (versione 2.8.1), pid 3801, utente 'root'

Oct 30 19:36:07 localhost gconfd (root-3801): L'indirizzo "xml:readonly:/etc/gconf/gconf.xml.mandatory" è stato risolta ad una fonte di configurazione in sola lettura in posizione 0

Oct 30 19:36:07 localhost gconfd (root-3801): L'indirizzo "xml:readwrite:/root/.gconf" è stato risolto ad una fonte di configurazione scrivibile in posizione 1

Oct 30 19:36:07 localhost gconfd (root-3801): L'indirizzo "xml:readonly:/etc/gconf/gconf.xml.defaults" è stato risolta ad una fonte di configurazione in sola lettura in posizione 2

Oct 30 19:36:16 localhost modem_run[3824]: modem_run version 1.3.1 started by root uid 0

lista dei moduli caricati (lsmode):

francesco:/home/francesco# lsmod

Module Size Used by

speedtch 14000 0

ds 17796 2

ipv6 229892 14

parport_pc 33348 0

lp 10408 0

parport 37320 2 parport_pc,lp

thermal 12944 0

fan 4236 0

button 6680 0

processor 17584 1 thermal

ac 5132 0

battery 9740 0

af_packet 20872 0

snd_via82xx 26660 0

snd_ac97_codec 59268 1 snd_via82xx

snd_pcm 85384 1 snd_via82xx

snd_timer 23300 1 snd_pcm

snd_page_alloc 11144 2 snd_via82xx,snd_pcm

gameport 4736 1 snd_via82xx

snd_mpu401_uart 7296 1 snd_via82xx

snd_rawmidi 23204 1 snd_mpu401_uart

snd_seq_device 7944 1 snd_rawmidi

snd 50660 7 snd_via82xx,snd_ac97_codec,snd_pcm,snd_timer,snd_mpu401_uart,snd_rawmidi,snd_seq_device

yenta_socket 19200 0

pcmcia_core 63028 2 ds,yenta_socket

pci_hotplug 30640 0

via_agp 8832 1

agpgart 31784 1 via_agp

ehci_hcd 27908 0

eth1394 19976 0

uhci_hcd 29328 0

via82cxxx_audio 26248 1

uart401 11460 1 via82cxxx_audio

sound 75308 2 via82cxxx_audio,uart401

soundcore 9824 4 snd,via82cxxx_audio,sound

ac97_codec 16908 1 via82cxxx_audio

via_rhine 19848 0

mii 4864 1 via_rhine

via_ircc 20368 0

irda 167360 1 via_ircc

crc_ccitt 2432 1 irda

ohci1394 32004 0

tsdev 7168 0

capability 4872 0

mousedev 9996 1

commoncap 7168 1 capability

joydev 9536 0

usbcore 104164 5 speedtch,ehci_hcd,uhci_hcd

evdev 9088 0

ppp_synctty 9472 0

ppp_generic 27540 1 ppp_synctty

slhc 7040 1 ppp_generic

sr_mod 15780 0

sbp2 22408 0

scsi_mod 115148 2 sr_mod,sbp2

ieee1394 100408 3 eth1394,ohci1394,sbp2

psmouse 17800 0

ide_cd 38176 0

cdrom 35740 2 sr_mod,ide_cd

ext3 109672 1

jbd 54552 1 ext3

ide_generic 1664 0

via82cxxx 12956 1

ide_disk 16768 3

ide_core 125028 4 ide_cd,ide_generic,via82cxxx,ide_disk

unix 26036 530

font 8576 0

vesafb 6688 0

cfbcopyarea 3840 1 vesafb

cfbimgblt 3200 1 vesafb

cfbfillrect 3712 1 vesafb

2005-10-30T02:08:22