Linux version 2.4.27-2-386 (horms@tabatha.lab.ultramonkey.org) (gcc version 3.3.5 (Debian 1:3.3.5-13)) #1 Wed Aug 17 09:33:35 UTC 2005

BIOS-provided physical RAM map:

BIOS-e820: 0000000000000000 - 000000000009fc00 (usable)

BIOS-e820: 000000000009fc00 - 00000000000a0000 (reserved)

BIOS-e820: 00000000000e0000 - 0000000000100000 (reserved)

BIOS-e820: 0000000000100000 - 000000001ffc0000 (usable)

BIOS-e820: 000000001ffc0000 - 000000001fff8000 (ACPI data)

BIOS-e820: 000000001fff8000 - 0000000020000000 (ACPI NVS)

BIOS-e820: 00000000fec00000 - 00000000fec01000 (reserved)

BIOS-e820: 00000000fee00000 - 00000000fee01000 (reserved)

BIOS-e820: 00000000ffb80000 - 00000000ffc00000 (reserved)

BIOS-e820: 00000000fff00000 - 0000000100000000 (reserved)

511MB LOWMEM available.

On node 0 totalpages: 131008

zone(0): 4096 pages.

zone(1): 126912 pages.

zone(2): 0 pages.

ACPI: RSDP (v000 AMI ) @ 0x000ff980

ACPI: RSDT (v001 GATEWA N0CPP063 0x20010820 MSFT 0x00001011) @ 0x1fff0000

ACPI: FADT (v001 GATEWA N0CPP063 0x20010820 MSFT 0x00001011) @ 0x1fff1000

ACPI: DSDT (v001 GATEWA N0CPP063 0x00000004 MSFT 0x0100000b) @ 0x00000000

Kernel command line: root=/dev/hda2 ro

Found and enabled local APIC!

Initializing CPU#0

Detected 1496.371 MHz processor.

Console: colour VGA+ 80x25

Calibrating delay loop... 2988.44 BogoMIPS

Memory: 512368k/524032k available (1069k kernel code, 11276k reserved, 459k data, 96k init, 0k highmem)

Dentry cache hash table entries: 65536 (order: 7, 524288 bytes)

Inode cache hash table entries: 32768 (order: 6, 262144 bytes)

Mount cache hash table entries: 512 (order: 0, 4096 bytes)

Buffer cache hash table entries: 32768 (order: 5, 131072 bytes)

Page-cache hash table entries: 131072 (order: 7, 524288 bytes)

CPU: Trace cache: 12K uops, L1 D cache: 8K

CPU: L2 cache: 256K

CPU: After generic, caps: 3febfbff 00000000 00000000 00000000

CPU: Common caps: 3febfbff 00000000 00000000 00000000

CPU: Intel(R) Pentium(R) 4 CPU 1500MHz stepping 07

Enabling fast FPU save and restore... done.

Enabling unmasked SIMD FPU exception support... done.

Checking 'hlt' instruction... OK.

Checking for popad bug... OK.

POSIX conformance testing by UNIFIX

enabled ExtINT on CPU#0

ESR value before enabling vector: 00000000

ESR value after enabling vector: 00000000

Using local APIC timer interrupts.

calibrating APIC timer ...

..... CPU clock speed is 1496.4229 MHz.

..... host bus clock speed is 99.7612 MHz.

cpu: 0, clocks: 997612, slice: 498806

CPU0<T0:997600,T1:498784,D:10,S:498806,C:997612>

ACPI: Subsystem revision 20040326

ACPI: Interpreter disabled.

PCI: PCI BIOS revision 2.10 entry at 0xfda95, last bus=2

PCI: Using configuration type 1

PCI: Probing PCI hardware

PCI: ACPI tables contain no PCI IRQ routing entries

PCI: Probing PCI hardware (bus 00)

Transparent bridge - Intel Corp. 82801BA/CA/DB/EB PCI Bridge

PCI: Using IRQ router PIIX/ICH [8086/2440] at 00:1f.0

Linux NET4.0 for Linux 2.4

Based upon Swansea University Computer Society NET3.039

Initializing RT netlink socket

Starting kswapd

VFS: Disk quotas vdquot_6.5.1

devfs: v1.12c (20020818) Richard Gooch (rgooch@atnf.csiro.au)

devfs: boot_options: 0x0

pty: 256 Unix98 ptys configured

Serial driver version 5.05c (2001-07-08) with HUB-6 MANY_PORTS MULTIPORT SHARE_IRQ SERIAL_PCI enabled

ttyS00 at 0x03f8 (irq = 4) is a 16550A

COMX: driver version 0.85 (C) 1995-1999 ITConsult-Pro Co. <info@itc.hu>

RAMDISK driver initialized: 16 RAM disks of 8192K size 1024 blocksize

Initializing Cryptographic API

NET4: Linux TCP/IP 1.0 for NET4.0

IP: routing cache hash table of 4096 buckets, 32Kbytes

TCP: Hash tables configured (established 32768 bind 65536)

Linux IP multicast router 0.06 plus PIM-SM

RAMDISK: cramfs filesystem found at block 0

RAMDISK: Loading 3708 blocks [1 disk] into ram disk... |#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#|#/#-#\#done.

Freeing initrd memory: 3708k freed

VFS: Mounted root (cramfs filesystem).

Freeing unused kernel memory: 96k freed

NET4: Unix domain sockets 1.0/SMP for Linux NET4.0.

Uniform Multi-Platform E-IDE driver Revision: 7.00beta4-2.4

ide: Assuming 33MHz system bus speed for PIO modes; override with idebus=xx

ide: late registration of driver.

ICH2: IDE controller at PCI slot 00:1f.1

ICH2: chipset revision 2

ICH2: not 100% native mode: will probe irqs later

ide0: BM-DMA at 0xffa0-0xffa7, BIOS settings: hda:DMA, hdb:DMA

ide1: BM-DMA at 0xffa8-0xffaf, BIOS settings: hdc:DMA, hdd:DMA

hda: WDC WD1200LB-22EDA0, ATA DISK drive

hdb: WDC AC310100B, ATA DISK drive

blk: queue e0825b60, I/O limit 4095Mb (mask 0xffffffff)

blk: queue e0825c9c, I/O limit 4095Mb (mask 0xffffffff)

hdc: LG CD-RW CED-8120B, ATAPI CD/DVD-ROM drive

hdd: LS-120 VER5 00 UHD Floppy, ATAPI FLOPPY drive

ide0 at 0x1f0-0x1f7,0x3f6 on irq 14

ide1 at 0x170-0x177,0x376 on irq 15

hda: attached ide-disk driver.

hda: 234441648 sectors (120034 MB) w/2048KiB Cache, CHS=14593/255/63, UDMA(100)

hdb: attached ide-disk driver.

hdb: 19807200 sectors (10141 MB) w/512KiB Cache, CHS=19650/16/63, UDMA(33)

Partition check:

/dev/ide/host0/bus0/target0/lun0: p1 p2 p3 < p5 p6 p7 p8 p9 p10 p11 p12 p13 >

/dev/ide/host0/bus0/target1/lun0: [PTBL] [1232/255/63] p1 p2 < p5 p6 p7 p8 p9 p10 p11 p12 p13 p14 > p3

Journalled Block Device driver loaded

kjournald starting. Commit interval 5 seconds

EXT3-fs: mounted filesystem with ordered data mode.

EXT3 FS 2.4-0.9.19, 19 August 2002 on ide0(3,2), internal journal

Real Time Clock Driver v1.10f

hdc: attached ide-cdrom driver.

hdc: ATAPI 32X CD-ROM CD-R/RW drive, 8192kB Cache, DMA

Uniform CD-ROM driver Revision: 3.12

SCSI subsystem driver Revision: 1.00

kjournald starting. Commit interval 5 seconds

EXT3 FS 2.4-0.9.19, 19 August 2002 on ide0(3,5), internal journal

EXT3-fs: mounted filesystem with ordered data mode.

kjournald starting. Commit interval 5 seconds

EXT3 FS 2.4-0.9.19, 19 August 2002 on ide0(3,6), internal journal

EXT3-fs: mounted filesystem with ordered data mode.

kjournald starting. Commit interval 5 seconds

EXT3 FS 2.4-0.9.19, 19 August 2002 on ide0(3,12), internal journal

EXT3-fs: mounted filesystem with ordered data mode.

kjournald starting. Commit interval 5 seconds

EXT3 FS 2.4-0.9.19, 19 August 2002 on ide0(3,13), internal journal

EXT3-fs: mounted filesystem with ordered data mode.

kjournald starting. Commit interval 5 seconds

EXT3 FS 2.4-0.9.19, 19 August 2002 on ide0(3,9), internal journal

EXT3-fs: mounted filesystem with ordered data mode.

kjournald starting. Commit interval 5 seconds

EXT3 FS 2.4-0.9.19, 19 August 2002 on ide0(3,7), internal journal

EXT3-fs: mounted filesystem with ordered data mode.

kjournald starting. Commit interval 5 seconds

EXT3 FS 2.4-0.9.19, 19 August 2002 on ide0(3,11), internal journal

EXT3-fs: mounted filesystem with ordered data mode.

kjournald starting. Commit interval 5 seconds

EXT3 FS 2.4-0.9.19, 19 August 2002 on ide0(3,10), internal journal

EXT3-fs: mounted filesystem with ordered data mode.

Adding Swap: 1951856k swap-space (priority -1)

Linux agpgart interface v0.99 (c) Jeff Hartmann

agpgart: Maximum main memory to use for agp memory: 439M

agpgart: Detected Intel i850 chipset

agpgart: AGP aperture is 64M @ 0xf8000000

usb.c: registered new driver usbdevfs

usb.c: registered new driver hub

usb-uhci.c: $Revision: 1.275 $ time 09:50:48 Aug 17 2005

usb-uhci.c: High bandwidth mode enabled

PCI: Found IRQ 5 for device 00:1f.2

PCI: Setting latency timer of device 00:1f.2 to 64

usb-uhci.c: USB UHCI at I/O 0xef40, IRQ 5

usb-uhci.c: Detected 2 ports

usb.c: new USB bus registered, assigned bus number 1

hub.c: USB hub found

hub.c: 2 ports detected

PCI: Found IRQ 9 for device 00:1f.4

PCI: Sharing IRQ 9 with 02:0b.0

PCI: Sharing IRQ 9 with 02:0c.2

PCI: Setting latency timer of device 00:1f.4 to 64

usb-uhci.c: USB UHCI at I/O 0xef80, IRQ 9

usb-uhci.c: Detected 2 ports

usb.c: new USB bus registered, assigned bus number 2

hub.c: USB hub found

hub.c: 2 ports detected

usb-uhci.c: v1.275:USB Universal Host Controller Interface driver

r8169 Gigabit Ethernet driver 1.2 loaded

PCI: Found IRQ 9 for device 02:0b.0

PCI: Sharing IRQ 9 with 00:1f.4

PCI: Sharing IRQ 9 with 02:0c.2

eth0: Identified chip type is 'RTL8169s/8110s'.

eth0: RTL8169 at 0xe0879c00, 00:08:54:28:41:95, IRQ 9

eth0: Auto-negotiation Enabled.

eth0: 100Mbps Full-duplex operation.

PCI: Found IRQ 9 for device 02:0c.2

PCI: Sharing IRQ 9 with 00:1f.4

PCI: Sharing IRQ 9 with 02:0b.0

usb-ohci.c: USB OHCI at membase 0xe09b8000, IRQ 9

usb-ohci.c: usb-02:0c.2, ALi Corporation USB 1.1 Controller (#3)

usb.c: new USB bus registered, assigned bus number 3

hub.c: USB hub found

hub.c: 2 ports detected

PCI: Found IRQ 3 for device 02:0c.1

usb-ohci.c: USB OHCI at membase 0xe09ba000, IRQ 3

usb-ohci.c: usb-02:0c.1, ALi Corporation USB 1.1 Controller (#2)

usb.c: new USB bus registered, assigned bus number 4

hub.c: USB hub found

hub.c: 2 ports detected

PCI: Found IRQ 11 for device 02:0c.0

PCI: Sharing IRQ 11 with 02:0d.0

PCI: Sharing IRQ 11 with 02:0d.1

usb-ohci.c: USB OHCI at membase 0xe09bc000, IRQ 11

usb-ohci.c: usb-02:0c.0, ALi Corporation USB 1.1 Controller

usb.c: new USB bus registered, assigned bus number 5

hub.c: USB hub found

hub.c: 2 ports detected

hub.c: new USB device 02:0c.1-1, assigned address 2

usb.c: USB device 2 (vend/prod 0x152e/0xe003) is not claimed by any active driver.

PCI: Found IRQ 10 for device 02:0c.3

PCI: Sharing IRQ 10 with 00:1f.3

ehci_hcd 02:0c.3: ALi Corporation USB 2.0 Controller

ehci_hcd 02:0c.3: irq 10, pci mem e09c3800

usb.c: new USB bus registered, assigned bus number 6

PCI: cache line size of 128 is not supported by device 02:0c.3

ehci_hcd 02:0c.3: USB 2.0 enabled, EHCI 1.00, driver 2003-Dec-29/2.4

hub.c: USB hub found

hub.c: 6 ports detected

usb.c: USB disconnect on device 02:0c.1-1 address 2

uhci.c: USB Universal Host Controller Interface driver v1.1

ich2rom: firmware access control, I can't enable writes

pci_hotplug: PCI Hot Plug PCI Core version: 0.5

shpchp: acpi_shpchprm:get_device PCI ROOT HID fail=0x1001

pci_hotplug: PCI Hot Plug PCI Core version: 0.5

pciehp: acpi_pciehprm:get_device PCI ROOT HID fail=0x1001

hub.c: new USB device 02:0c.3-3, assigned address 2

usb.c: USB device 2 (vend/prod 0x152e/0xe003) is not claimed by any active driver.

i810_rng hardware driver 0.9.8 loaded

hw_random: misc device register failed

Initializing USB Mass Storage driver...

usb.c: registered new driver usb-storage

scsi0 : SCSI emulation for USB Mass Storage devices

Vendor: HL-DT-ST Model: DVDRAM GSA-5163D Rev: A103

Type: CD-ROM ANSI SCSI revision: 02

Attached scsi CD-ROM sr0 at scsi0, channel 0, id 0, lun 0

sr0: scsi-1 drive

WARNING: USB Mass Storage data integrity not assured

USB Mass Storage device found at 2

USB Mass Storage support registered.

apm: BIOS version 1.2 Flags 0x03 (Driver version 1.16)

parport0: PC-style at 0x378 (0x778) [PCSPP,TRISTATE]

parport0: irq 7 detected

parport0: faking semi-colon

parport0: Printer, Hewlett-Packard HP LaserJet 2100 Series

lp0: using parport0 (polling).

spurious 8259A interrupt: IRQ7.

Maloclm Jordan

2006-06-28T17:14:43